#
NO.29 DOES NOT SHIFT UP IN M RANGE [JA5AX-EL]

id050305809100

29 | Does not shift up in M range
DESCRIPTION | • Gear position indicator light in instrument cluster illuminates, but vehicle does not upshift when selector lever is pushed to "+" side.
POSSIBLE CAUSE | • Up switch or related harness malfunction Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.