IMMOBILIZER SYSTEM COMPONENT REPLACEMENT/KEY ADDITION AND CLEARING [WITH ADVANCED KEYLESS SYSTEM]

id0914z68050b2

Foreword

• When performing the following procedures, the immobilizer resetting procedure using the WDS or equivalent must also always be performed: “Keyless control module replacement”, “PCM replacement”, “Steering lock unit replacement”, “Keyless control module and PCM joint replacement”, “Keyless control module, PCM, and steering lock unit joint replacement”, and “Key ID number clearing”. The engine will not start unless all work is performed using the WDS or equivalent.
• A card key that can start the engine is necessary for the key programming. If there is no card key that can start the engine, perform the key programming after the card key programming. (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)
• There are two ways to add supplemental key: Using the WDS or equivalent or using two keys that can start the engine to program.
• When replacing any of the immobilizer system component parts, adding/clearing keys, or performing other functions, refer to the following table and perform the applicable procedure (No.1 to 6).
• Verify that the room fuse is equipped.

Ref. No. | Condition | Items necessary for procedure (prepare before starting procedure) | Cautionary notes
--- | --- | --- | ---
1 | Since two or more keys that can start the engine are necessary, make a spare key. Or program an additional key. | • Programming key | • The WDS or equivalent is necessary for the additional key programming if “Customer spare key programming disable” is performed before the procedure using the WDS or equivalent. In this case, perform No. 2.
2 | If there is only one key that can start the engine, make a spare key. If there is no key, program an additional key. | • Programmed card key • Programming key • WDS or equivalent | -
3 | Clearing the programmed key ID number. | • Programming keys (two or more) • WDS or equivalent | • The key ID number programmed to the vehicle will be completely cleared. • The engine cannot be started unless the key is reprogrammed after the procedure. Before beginning the procedure, verify that the customer has turned in all of the keys for the vehicle. • The engine cannot be started unless two or more keys are reprogrammed after the procedure. • The two or more keys prepared before the procedure do not have to be new ones and there is no problem with using the key that was used to start the engine before the procedure.
3 | Replacing all the keys. (Steering lock unit is not replaced) | • Programmed card key • Programming keys (two or more) • WDS or equivalent | • The keys (two or more) prepared before the procedure do not have to be new ones, and there is no problem with using the key that was used to start the engine before the procedure. • The engine cannot be started unless the key is reprogrammed after the procedure.
3 | Replacing the PCM only. | • New PCM • Programmed card key • Programming keys (two or more) • WDS or equivalent | -
4 | Changing the additional key programming procedure. (Method for programming other keys using two keys that can start the engine is disabled.) | • WDS or equivalent | • The additional key programming using No. 1 cannot be performed after the procedure. It is possible to restore the setting. For restoring the setting, the WDS or equivalent is necessary.
4 | Changing the additional key programming procedure. Allows programming using two keys that can start the engine. | • WDS or equivalent | • New vehicles have this setting.
5 | Replacing the steering lock unit only. | • New steering lock unit • Programmed card key • New keys (two or more) • WDS or equivalent | • Have two or more keys ready for programming before beginning the procedure, since the previous keys will be invalid. • The steering lock unit programming is necessary for the keyless control module before the key programming. • Two or more keys need to be programmed after the procedure to start the engine.
5 | Replacing the PCM and steering lock unit at the same time. | • New PCM • New steering lock unit • Programmed card key • New keys (two or more) • WDS or equivalent | • Have two or more keys ready for programming before beginning the procedure, since the previous keys will be invalid. • Perform the steering lock unit programming. • Two or more keys need to be programmed after the procedure to start the engine.
5 | Replacing the keyless control module only. | • New keyless control module • Programming card key • Programming keys (two or more) • WDS or equivalent | • Unless keys are reprogrammed after the procedure, the engine cannot be started. Before beginning the procedure, verify that the customer has turned in all of the card keys and keys for the vehicle. • Perform the card key programming. • Perform the steering lock unit programming. • Unless card keys and keys (two or more) are programmed after the procedure, the engine cannot be started. • The card key and keys (two or more) prepared before the procedure do not have to be new ones and there is no problem with using the keys that were used to start the engine before the procedure.
5 | Replacing the keyless control module and steering lock unit at the same time. | • New keyless control module • New steering lock unit • Programming card key • New keys (two or more) • WDS or equivalent | • Unless keys are re-programmed after the procedure, the engine cannot be started. Before beginning the procedure, verify that the customer has turned in all of the card keys and keys for the vehicle. • Perform the card key programming. • Perform the steering lock unit programming. • The engine cannot be started unless a card key and keys (two or more) are programmed. • The card key and keys (two or more) prepared before the procedure do not have to be new ones and there is no problem with using the keys that were used to start the engine before the procedure.
5 | Replacing the PCM and keyless control module at the same time. | • New PCM • New keyless control module • Programming card key • Programming keys (two or more) • WDS or equivalent | • Unless keys are reprogrammed after the procedure, the engine cannot be started. Before beginning the procedure, verify that the customer has turned in all of the card keys and keys for the vehicle. • Perform the card key programming. • Perform the steering lock unit programming. • The engine cannot be started unless a card key and two or more keys are programmed after the procedure. • The card key and keys (two or more) prepared before the procedure do not have to be new ones and there is no problem with using the keys that were used to start the engine before the procedure.
5 | Replacing the PCM, keyless control module, and steering lock unit at the same time. | • New PCM • New keyless control module • New steering lock unit • Programming card key • Programming keys (two or more) • WDS or equivalent | • Unless keys are reprogrammed after the procedure, the engine cannot be started. Before beginning the procedure, verify that the customer has turned in all of the card keys and keys for the vehicle. • Perform the card key programming. • Perform the steering lock unit programming. • The engine cannot be started unless a card key and two or more keys are programmed after the procedure. • The card key and keys (two or more) prepared before the procedure do not have to be new ones and there is no problem with using the keys that were used to start the engine before the procedure.
6 | Program the keys(There is no programmed key or programmed card key) | • Programming card key • Programming keys (two or more) • M-MDS | -
- | Replacing the coil antenna. | • New coil antenna | • Immobilizer system resetting is not necessary.

  Caution
  • The following conditions may cause poor signal communication between the key and vehicle, resulting in the engine not starting or a key registration error. Do not perform any work under the following conditions:
    ― Placing the following items close to the key grip or contacting it.
      • Spare keys
      • Keys for other vehicles equipped with an immobilizer system
      • Any metallic object
      • Any electronic device, or any credit or other card with magnetic strips
  • Do not place the following devices in the vehicle while programming, otherwise programming cannot be performed:
    ― WDS or equivalent
    ― Personal computer
    ― Devices that can send/receive the radio waves

  Note
  • The “valid key” used in this manual indicates the key that can start the engine.
  • If the key adding, programming, clearing, and immobilizer system construction parts replacement are performed, verify that the all keys can start the engine within 5 s after the procedure.
  • When verifying that the engine starts, wait at least 5 s or more before starting the engine using the next key.
  • If the engine cannot be started using a programmed key, repeat the procedure from the beginning.
  • Do not start the engine unless indicated in the procedure. If the engine is started during the programming procedure, programming is stopped at that point. Repeat the procedure starting from the beginning if the engine is started before completion.
  • Do not place the card key in the vehicle or bring it within approx. 1 m of the vehicle unless indicated in the procedure.
  • Two or more key ID numbers must be programmed for the engine to start.
  • A maximum of eight key ID numbers can be programmed for one vehicle. The WDS or equivalent can be used to verify the number of key ID numbers programmed to a single vehicle.
  • Do not select a WDS or equivalent screen menu other than one indicated in the procedure.

WDS or Equivalent Connecting Procedure

  Caution
  • Do not place the WDS or equivalent in the vehicle while programming, otherwise programming cannot be performed.

1. Fully lower the door glass.

2. Connect the WDS or equivalent to the DLC-2.

am6zzw00014662

3. Pull out the WDS or equivalent cable from the door glass opening and set the WDS or equivalent outside the vehicle.

  Caution
  • Protect the cable and body contact area with a clean rag, otherwise they could be damaged.

No.1 Additional Key Programming Procedure (Using Two Valid Keys)

  Caution
  • Do not place the following devices in the vehicle while programming, otherwise programming cannot be performed:
    ― Card key
    ― WDS or equivalent
    ― Personal computer
    ― Devices that can send/receive the radio waves

Condition
• Have two or more valid keys.

  Note
  • A maximum of eight keys can be programmed for one vehicle. If key programming is not successful and DTC 15 appears even though the procedure was performed properly, use the PID/data monitor function of the WDS or equivalent and verify the number of keys that have been programmed.
  • If eight keys have already been programmed, and it is necessary to program other keys, the previously programmed key ID numbers must first be cleared. To clear the key, refer to “No.3 PCM, and Key Replacement Procedure (Clearing Previously Programmed Key ID Numbers, Key Re-program)”.

Procedure

am6zzw00014663

1. Prepare key 3 for programming.

2. Start the engine using key 1.

3. Verify that the security light illuminates for approx. 3 s, and then goes out.

4. Turn the ignition switch to the LOCK position.

5. Using key 1, turn the ignition switch to the ON position.

6. Verify that the security light illuminates for approx. 3 s, and then goes out.

7. Using key 1, turn the ignition switch to the LOCK position within approx. 4 s after the security light goes out.

8. Remove key 1.

9. Repeat Steps 2—5 using key 2 instead of key 1.

10. Repeat Steps 5—8 using key 3 instead of key 1.

11. If additional keys need to be programmed, repeat Steps 1—10, and replace key 3 in Step 10 with the key to be programmed (key 4).

No. 2 Key Additional Programming Procedure (Using the WDS or Equivalent)

Condition
• There is only one valid key. Or, there is no valid key but there is a card key that can start the engine.

  Note
  • A maximum of eight keys can be programmed for one vehicle. If key registration is not successful and DTC 15 appears even though the procedure was performed properly, use the PID/data monitor function of the WDS or equivalent and verify the number of keys that have been programmed.
  • If eight keys have already been programmed, and it is necessary to program other keys, the previously programmed key ID numbers must first be cleared. To clear the key ID number, refer to “No.3 PCM, and Key Replacement Procedure (Clearing Previously Programmed Key ID Numbers, Key Re-program)”.

Procedure

1. Prepare key 1 for programming.

2. Start the engine using a valid key or card key.

  Caution
  • Do not place the card key in the vehicle when starting the engine with the valid key, otherwise programming cannot be performed. If the engine is started with the card key, remove the card key from the vehicle after the engine is started.

3. Verify that the security light illuminates for approx. 3 s, and then goes out.

4. Turn the ignition switch to the LOCK position.

5. Connect the WDS or equivalent to the DLC-2. (See WDS or Equivalent Connecting Procedure.)

6. Using key 1, turn the ignition switch to the ON position.

  Note
  • Although the security light flashes and DTC 15 is displayed, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

7. Select “BODY/SECURITY/PATS (immobilizer) function” from the WDS or equivalent screen menu.

8. Select “Ignition key additional programming” from the WDS or equivalent screen menu.

  Note
  • After selecting the above menu, “operation is successful” is displayed. At this point, the key that turned the ignition switch to the ON position is completely programmed.

  • In this procedure, the necessary number of the keys are completely programmed. To finish the additional key programming, go to Step 13.
  • If additional keys need to be programmed, go to the next step.

9. Perform the security access according to the directions on the WDS or equivalent screen. (See SECURITY ACCESS PROCEDURE.)

10. After verifying that the PATS function menu is displayed again on the WDS or equivalent screen, turn the ignition switch to the LOCK position and remove key 1.

11. Using the key to be programmed, turn the ignition switch to the ON position.

12. Return to the Step 6.

13. After verifying that the PATS function menu is displayed again on the WDS or equivalent screen, select the “Finish (this menu)” to finish the WDS or equivalent procedure.

14. After Step 10, wait 5 s or more, and then turn the ignition switch to the LOCK position.

No.3 PCM, and Key Replacement Procedure (Clearing Previously Programmed Key ID Numbers, Key Re-program)

Condition
• Have two or more keys to be programmed after the key ID number clearing.

  Caution
  • Before starting Step 1, complete the procedure for PCM replacement.

Procedure

am6zzw00014664

1. Prepare two or more keys to be programmed after the key ID number clearing.

2. Connect the WDS or equivalent to the DLC-2. (See WDS or Equivalent Connecting Procedure.)

3. Using key 1, turn the ignition switch to the ON position.

  Note
  • Although the security light flashes and DTC 15 or 21 is displayed, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

4. Verify that the keyless warning light illuminates for approx. 3 s, and then goes out.

5. Select “BODY/SECURITY/PATS (immobilizer) function” from the menu.

6. Select “Ignition key ID number Clearing” from the WDS or equivalent screen menu and perform the procedure according to the WDS or equivalent screen.

7. Perform the security access according to the direction of the WDS or equivalent screen. (See SECURITY ACCESS PROCEDURE.)

8. After verifying that the PATS function menu is displayed again on the WDS or equivalent screen, select “Finish (this menu)” to finish the WDS or equivalent procedure.

9. After Step 9, wait 5 s or more, and then turn the ignition switch to the LOCK position.

10. Using key 1, turn the ignition switch to the ON position.

11. After verifying that the security light and keyless warning light illuminates for 3 s or more turn the ignition switch to the LOCK position and remove key 1.

  Note
  • Although the security light flashes and DTC 21 is displayed, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

12. Using key 2, turn the ignition switch to the ON position.

13. Verify that the security light and keyless warning light illuminates for approx. 3 s, and then goes out.

14. After verifying that the security light goes out, turn the ignition switch to the LOCK position using key 2, and then remove key 2.

15. If an additional key needs to be programmed, repeat Steps 13—15 with the additional key being key 3. If the ignition switch is held in the ON position for 1 min or more, the additional key programming procedure according to Steps 13—15 will not be possible. If this occurs, refer to “No.1 Additional Key Programming Procedure (Using Two Valid Keys)” to register any additional keys.

16. Start the engine with the key 1.

17. Verify that the security light and keyless warning light operate as follows:

  • From the point when the ignition switch is turned to the ON position, the security light illuminates for approx. 3 s and goes out.
  • The keyless warning light illuminates with the ignition switch turned to the ON position, and after approx. 1 s after the engine is started, it goes out and displays the number of programmed keys.

  e6u914zw1026

18. After verifying that the keyless warning light goes out, turn the ignition switch to the LOCK position using key 1.

19. Repeat Steps 17—19 using key 2 instead of key 1.

  Note
  • Perform Steps 17—19 as well when there are three or more programmed keys.

20. Start the engine with the card key and remove any key from the key cylinder.

  Caution
  • Remove any key from the key cylinder.

21. Verify that the security light and keyless warning light operate as follows:

  • From the point when the ignition switch is turned to the ON position, the security light illuminates for approx. 3 s, and goes out.
  • The keyless warning light illuminates when the ignition switch is turned to the ON position, and after approx. 1 s after the engine is started, it goes out.

22. Turn the ignition switch to the LOCK position after verifying that the keyless warning light goes out.

No. 4 Key Additional Programming Procedure Changing

  Note
  • This procedure is performed for enabling/diabling the “No.1 Additional Key Programming Procedure (Using Two Valid Keys)” setting.
  • This procedure is possible when the vehicle is new, and when replacing the keyless unit with a new one.
  • If “No.1 Additional Key Programming Procedure (Using Two Valid Keys)” is set to disable, the additional key programming can be only performed using the WDS or equivalent preventing the forging of a spare key by using two keys that can start the engine. This function is for use by rental car agencies or other companies with vehicle fleets.

Procedure

1. Using the key, turn the ignition switch to the ON position. (The key can be either the valid key or an unprogrammed key)

  Note
  • Although the security light flashes and DTC 15 is displayed when an unprogrammed key is used, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

2. Connect the WDS or equivalent to the DLC-2.

3. Select “BODY/SECURITY/PATS (immobilizer) function” from the WDS or equivalent screen menu.

4. Select “Customer spare key programming enable” or “Customer spare key programming disable” from the WDS or equivalent screen menu. The key additional programming procedure is as follows according to the selected menu:

Setting | Additional key programming procedure
--- | ---
Method using two valid keys | Method using the WDS or equivalent
Customer spare key programming enable | – | –
Customer spare key programming disable | × | –

? :Available
× :Unavailable

5. Perform the security access according to the directions on the WDS or equivalent screen. (See SECURITY ACCESS PROCEDURE.)

6. After verifying that the PATS function menu is displayed again on the WDS or equivalent screen, select “Finish (this menu)” to finish the WDS or equivalent procedure.

7. After Step 6, wait 5 s or more and then turn the ignition switch to the LOCK position.

No.5 Resetting Procedure for the Immobilizer System when Replacing the PCM, Keyless Control Module, or Steering Lock Unit

Condition
• When the keyless control module is replaced

  ― Have one or more card keys to be programmed after the replacement.
  ― Have two or more keys to be programmed after the replacement.

• When the keyless control module is not to be replaced

  ― Have one or more card keys to be programmed.
  ― Have two or more keys to be programmed after the replacement.

  Caution
  • Perform the procedures in the following order: “Key ID number clearing”, “Card key programming”, “Steering lock unit programming”, and “Key programming”. If there is a failure in the programming, the engine may not be started.
  • When replacing only the PCM, start from Step 2. Key 1 in the procedure can be any valid key.
  • Perform the “card key programming procedure” in Step 9 only when the keyless control module is replaced.
  • Perform the “steering lock unit programming procedure” in Step 10 only when either the keyless control module or steering lock unit is replaced.

Procedure

am6zzw00014664

1. Prepare two or more keys to be programmed after the key ID number is cleared.

2. Connect the WDS or equivalent to the DLC-2. (See WDS or Equivalent Connecting Procedure.)

3. Using key 1, turn the ignition switch to the ON position.

  Note
  • Although the security light flashes and DTC 15 or 21 is displayed, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

4. Verify that the keyless warning light illuminates for approx. 3 s and then goes out.

5. Select “BODY/SECURITY/PATS (immobilizer) function” from the WDS or equivalent screen menu.

6. Select “Ignition key ID number clearing” from the WDS or equivalent screen menu and perform the procedure according to the WDS or equivalent screen.

7. Perform the security access according to the directions on the WDS or equivalent screen. (See SECURITY ACCESS PROCEDURE.)

  Caution
  • The WDS or equivalent displays “At least two or more keys must be programmed”, however, do not perform the key programming and proceed to Step 8 or 9. If the procedure is not followed, the engine may not be started.
  The key programming procedure is performed at Step 12—15.

8. Perform the card key programming. (when the keyless control module is replaced) (See CARD KEY ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)

9. Perform the steering lock unit programming. (when either the keyless control module or steering lock unit is replaced) (See STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM].)

10. After verifying that the PATS function menu is displayed again on the WDS or equivalent screen, select “Finish (this menu)” to finish the WDS or equivalent procedure.

11. After Step 11, wait 5 s or more and then turn the ignition switch to the LOCK position.

12. Using key 1, turn the ignition switch to the ON position.

13. After verifying that the security light and keyless warning light illuminate for 3 s or more, turn the ignition switch to the LOCK position and remove key 1.

  Note
  • Although the security light flashes and DTC 21 is displayed, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

14. Using key 2, turn the ignition switch to the ON position.

15. Verify that the security light and keyless warning light illuminate for approx. 3 s, and then goes out.

16. After verifying that the security light goes out, turn the ignition switch to the LOCK position using key 2, and then remove key 2.

17. If additional keys need to be programmed, repeat Steps 15—17 with the additional key to be programmed being key 3. If the ignition switch is held in the ON position for 1 min or more, additional key programming according to Steps 15—17 will not be possible. If this occurs, refer to “No.1 Additional Key Programming Procedure (Using Two Valid Keys)” to program any additional keys.

18. Start the engine with key 1.

19. Verify that the security light and keyless warning light operate as follows:

  • From the point when the ignition switch is turned to the ON position, the security light illuminates for approx. 3 s, and goes out.
  • The keyless warning light illuminates when the ignition switch is turned to the ON position, and the light goes out after approx. 1 s, and then displays the number of the programmed keys.

  e6u914zw1026

20. After verifying that the keyless warning light goes out, turn the ignition switch to the LOCK position using key 1, and then remove the key.

21. Repeat Steps 19—21 using key 2 instead of key 1.

  Note
  • Perform Steps 19—21 as well when three or more keys are to be programmed.

22. Start the engine using the card key.

  Caution
  • Remove any key from the key cylinder.

23. Verify that the security light and keyless warning light operate as follows:

  • From the point that ignition switch is turned to the ON position, the security light illuminates for approx. 3 s, and goes out.
  • The keyless warning light illuminate when the ignition switch is turned to the ON position for approx. 1 min, and goes out.

24. After verifying that the keyless warning light goes out, turn the ignition switch to the LOCK position.

No.6 Key Programming Procedure (If there is no programmed key or programmed advanced key)

Condition
• Have two or more keys to be programmed.
• Have one or more card keys to be programmed.

Procedure

1. Fully lower the driver-side door glass.

2. Connect the M-MDS to the DLC-2.

3. Pull out the M-MDS cable from the door glass opening and set the M-MDS outside the vehicle.

  Caution
  • Protect the cable and body contact area with a clean rag, otherwise they could be damaged.

4. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (notebook PC)
    1. Select “Body”.
    2. Select “Security”.

  • When using the PDS (pocket PC)
    1. Select “Programming”.

5. Then, select items from the screen menu in the following order.

  1. Select “PATS functions”.
  2. Select “Card Key Code Erase”.

6. Security access begins and the M-MDS displays the “OUT-CODE”.

  Note
  When “OUT-CODE” is first displayed, turning the ignition switch from the LOCK to the ON position 5 times will change the “OUT-CODE”.

7. Input the “IN-CODE” that corresponds to the “OUT-CODE” displayed in the M-MDS screen.

8. Select “CARD KEY CLEARING” from the M-MDS screen menu.

9. Then, select the following items from the initialization screen of the M-MDS.

  • When using the IDS (notebook PC)
    1. Select “Body”.
    2. Select “Security”.

  • When using the PDS (pocket PC)
    1. Select “Programming”.

10. Then, select items from the screen menu in the following order.

  1. Select “PATS functions”.
  2. Select “Program Additional Card Key”.

11. Security access begins and the M-MDS displays the “OUT-CODE”.

  Note
  • When “OUT-CODE” is first displayed, turning the ignition switch from the LOCK to the ON position 5 times will change the “OUT-CODE”.

12. Input the “IN-CODE” that corresponds to the “OUT-CODE” displayed on the M-MDS screen.

13. Select “CARD KEY PROGRAMMING” from the M-MDS screen menu.

  Note
  • After Step 13 is completed and the card key programming is activated, the door lock actuator operates to lock, and then operates to unlock.

14. Press the unprogrammed card key UNLOCK button twice.

  Note
  • After Step 14 is completed and the card key is programmed, the door lock actuator operates to lock, and then operates to unlock.

15. If programming more card keys, remove the supplementary key once, and then repeat the procedure from Step 12 by following the instructions on the M-MDS screen.

  Caution
  • Do not place the card key in the vehicle when starting the engine with the valid key, otherwise programming cannot be performed. If the engine is started with the card key, remove the card key from the vehicle after the engine is started.

16. After verifying that the PATS function menu is displayed again on the WDS or equivalent screen, select “Finish (this menu)” to finish the WDS or equivalent procedure.

17. After Step 16, wait 5 s or more and then turn the ignition switch to the LOCK position.

18. Using key 1, turn the ignition switch to the ON position.

19. After verifying that the security light and keyless warning light illuminate for 3 s or more, turn the ignition switch to the LOCK position and remove key 1.

  Note
  • Although the security light flashes and DTC 21 is displayed, this does not indicate an improper procedure. Continue to perform the procedure as indicated.

20. Using key 2, turn the ignition switch to the ON position.

21. Verify that the security light and keyless warning light illuminate for approx. 3 s, and then goes out.

22. After verifying that the security light goes out, turn the ignition switch to the LOCK position using key 2, and then remove key 2.

23. If additional keys need to be programmed, repeat Steps 20—22 with the additional key to be programmed being key 3. If the ignition switch is held in the ON position for 1 min or more, additional key programming according to Steps 20—22 will not be possible. If this occurs, refer to “No. 2 Key Additional Programming Procedure (Using the WDS or Equivalent)” to program any additional keys.

24. Start the engine with key 1.

25. Verify that the security light and keyless warning light operate as follows:

  • From the point when the ignition switch is turned to the ON position, the security light illuminates for approx. 3 s, and goes out.
  • The keyless warning light illuminates when the ignition switch is turned to the ON position, and the light goes out after approx. 1 s, and then displays the number of the programmed keys.

  e6u914zw1026

26. After verifying that the keyless warning light goes out, turn the ignition switch to the LOCK position using key 1, and then remove the key.

27. Repeat Steps 24—26 using key 2 instead of key 1.

  Note
  • Perform Steps 24—26 as well when three or more keys are to be programmed.

28. Start the engine using the card key.

  Caution
  • Remove any key from the key cylinder.

29. Verify that the security light and keyless warning light operate as follows:

  • From the point that ignition switch is turned to the ON position, the security light illuminates for approx. 3 s, and goes out.
  • The keyless warning light illuminate when the ignition switch is turned to the ON position for approx. 1 min, and goes out.

30. After verifying that the keyless warning light goes out, turn the ignition switch to the LOCK position.