#
INSTRUMENT CLUSTER REMOVAL/INSTALLATION

id092200800500

  Caution

  • When replacing the instrument cluster, the configuration procedure must be performed before removing the instrument cluster. If the configuration procedure is not performed before removing the instrument cluster, it is possible that the instrument cluster will not operate normally.

1. Configurate the instrument clutter (when only replacing it). (See INSTRUMENT CLUSTER CONFIGURATION.)

2. Disconnect the negative battery cable.

3. Pull down the adjusting lever of the tilt steering wheel and push the steering wheel down.

4. Pull the steering wheel toward you.

5. Remove the meter hood.

6. Remove in the order indicated in the table.

1 | Screw
2 | Connector
3 | Instrument cluster (See Instrument Cluster Removal Note)

7. Install in the reverse order of removal.

## Instrument Cluster Removal Note

1. When removing the instrument cluster, in order to prevent damage to the lens, cover the steering shaft with a cloth.