#
COMMON RAIL INSPECTION [MZR-CD (RF Turbo)]

id0114f1803800

  Caution

  • Do not remove the fuel pressure sensor nor the fuel pressure limiter from the common rail. Since fuel pressure in the common rail is extremely high, the fuel pressure sensor, fuel pressure limiter, or the common rail can be damaged, leading to fuel leakage if any of them are removed.

1. Visually inspect the common rail for damage and cracks. Also verify that there is no extreme rust which will cause fuel leakage.

  • If either is observed, replace the common rail.