#
HEADLIGHT CLEANER MOTOR REMOVAL/INSTALLATION

id091900803300

1. Disconnect the negative battery cable.

2. Remove the washer tank. (See WASHER TANK REMOVAL/INSTALLATION.)

3. Remove the washer fluid-level sensor. (See WASHER FLUID-LEVEL SENSOR REMOVAL/INSTALLATION.)

4. Remove in the order indicated in the table.

1 | Connector
2 | Bolt
3 | Bracket
4 | Headlight cleaner motor
5 | Grommet

5. Install in the reverse order of removal.