#
SIMULATION FUNCTION [JA5AX-EL]

id050206100800
• By using the WDS or equivalent, simulation items for input/output parts preset in the TCM can be optionally selected and operated regardless of TCM control conditions.

Simulation item table

X: Available

Simulation item | Applicable component | Unit/Condition | Operation | PCM terminal
--- | --- | --- | --- | ---
IG ON | Idle
24B_Duty | 2-4 brake solenoid valve control signal in TCM | % |  | X | 2V
HC_Duty | High clutch solenoid valve control signal in TCM | % |  | X | 2U
LPS | Pressure control solenoid control signal in TCM | % |  | X | 2Y
NSFT TIM | Neutral shift solenoid valve control signal in TCM | On/Off |  | X | 2D
RDCN TIM | Reduction timing solenoid valve control signal in TCM | On/Off |  | X | 2G
SSA/SS1 | Shift solenoid A control signal in TCM | On/Off |  | X | 2W
SSB/SS2 | Shift solenoid B control signal in TCM | On/Off |  | X | 2T
SSC/SS3 | Shift solenoid C control signal in TCM | On/Off |  | X | 2X
TCCC | TCC solenoid valve control signal in TCM | % |  | X | 2S