#
DTC P0117 [L3 Turbo]

id0102b7804000

DTC P0117 | ECT sensor circuit low input
--- | ---
DETECTION CONDITION | • The PCM monitors the ECT sensor signal. If the PCM detects the ECT sensor voltage below 0.2 V, the PCM determines that the ECT sensor circuit has a malfunction. Diagnostic support note • This is a continuous monitor (Engine cooling system). • The MIL illuminates if the PCM detects the above malfunction condition during first drive cycle. • FREEZE FRAME DATA is available. • DTCs are stored in the PCM memory.
POSSIBLE CAUSE | • ECT sensor malfunction • Connect or terminal malfunction • Short to ground in the wiring harness between ECT sensor terminal A and PCM connector terminal 1M • Short to each wiring harness in ECT signal circuit and ECT ground circuit • PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA AND DIAGNOSTIC MONITORING TEST RESULTS HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Information availability. • Is any related Service Information available? | Yes | Perform repair or diagnosis according to the available Service information. If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT FOR BENT TERMINALS • Turn the ignition switch off. • Disconnect the ECT sensor connector. • Inspect ECT sensor terminals A and B (part-side) for bending. • Is there any malfunction? | Yes | Repair or replace the terminal, then go to Step 7.
No | Go to the next step.
4 | CLASSIFY ECT SENSOR MALFUNCTION OR WIRING HARNESS MALFUNCTION • Connect the WDS or equivalent to DLC-2. • Access the ECT PID. • Verify the ECT value when disconnecting the ECT sensor connector. • Does the ECT value change? | Yes | Replace the ECT sensor, then go to Step 7. (See ENGINE COOLANT TEMPERATURE (ECT) SENSOR REMOVAL/INSTALLATION [L3 Turbo].)
No | Go to the next step.
5 | INSPECT ECT SIGNAL CIRCUIT FOR SHORT TO GROUND • Turn the ignition switch off. • Inspect for continuity between ECT sensor terminal A (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness for a short to ground, then go to Step 7.
No | Go to the next step.
6 | INSPECT ECT CIRCUIT FOR SHORT TO WIRING HARNESSES • Inspect for continuity between ECT sensor terminal A and B (wiring harness-side). • Is there continuity? | Yes | Repair or replace the wiring harness for a short, then go to the next step.
No | Go to the next step.
7 | VERIFY TROUBLESHOOTING OF DTC P0117 COMPLETED • Make sure to reconnect all disconnected connectors. • Clear the DTC from the PCM memory using the WDS or equivalent. • Start the engine. • Is the same DTC present? | Yes | Replace the PCM, then go to the next step. (See PCM REMOVAL/INSTALLATION [L3 Turbo].)
No | Go to the next step.
8 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [L3 Turbo].) • Are any DTCs present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [L3 Turbo].)
No | Troubleshooting completed.