#
FRONT OUTER HANDLE REMOVAL/INSTALLATION

id0914z6432300

1. Remove the front door glass.

2. Detach the outer handle and front door latch rod.

3. For protector-equipped vehicles, refer to key cylinder removal/installation to remove the protector.

4. Remove the bolts.

5. With the rear side of the outer handle fixed and the outer handle lever pulled out (1), remove the rear side of the outer handle from the front door.

6. Pull out the front side of the outer handle from the front door.

7. Remove the request switch harness from the door. (with advanced keyless system)

8. Install in the reverse order of removal.