#
REAR WIPER SYSTEM OPERATION

id091900100900

## Continuous Operation

• When the rear wiper switch is moved to the ON position, current flows to the rear wiper relay, turning it on.
• When the rear wiper relay turns on, current flows to the rear wiper motor due to a control signal from the microcomputer and the wiper operates continuously.
• When the rear wiper switch is returned to the OFF position, the auto-stop function activates and the wiper stops at the park position.

.

1 | Microcomputer
2 | Rear wiper motor
3 | Auto-stop switch
4 | Rear washer motor
5 | Rear washer switch
6 | Rear wiper and washer switch

## Autostop Operation

• When the rear wiper switch is turned to the OFF position while the wiper is operating, current flows to the autostop switch, which is on, and the rear wiper motor operates until it returns to the park position, stopping the wiper.

.

1 | Microcomputer
2 | Rear wiper motor
3 | Auto-stop switch
4 | Rear washer motor
5 | Rear washer switch
6 | Rear wiper and washer switch

## Intermittent Wiper Operation

• When the rear wiper switch is moved to the INT position, current (1) flows.
• The microcomputer in the PJB flows current at 10 s intervals and the rear wiper relay is intermittently energized.
• As a result, current (2) flows at 10 s intervals causing the rear wiper to operate intermittently.
• When the rear wiper switch is moved to the OFF position while the wiper is operating, the rear wiper motor performs an auto-stop and stops in the park position.

.

1 | Microcomputer
2 | Rear wiper motor
3 | Auto-stop switch
4 | Rear washer motor
5 | Rear washer switch
6 | Rear wiper and washer switch

## Synchronized Washer And Wiper Operation

• When the rear wiper switch is turned upward from the ON position, current (2) flows, the rear washer motor operates and washer fluid is sprayed from the rear washer nozzle.

1 | Microcomputer
2 | Rear wiper motor
3 | Auto-stop switch
4 | Rear washer motor
5 | Rear washer switch
6 | Rear wiper and washer switch

• While turning the rear wiper switch downward from the OFF position, current (2) flows, the rear washer motor operates and washer fluid is sprayed from the rear washer nozzle. Current (1) flows at the same time according to the control signal from the microcomputer and the rear wiper motor operates continuously.

1 | Microcomputer
2 | Rear wiper motor
3 | Auto-stop switch
4 | Rear washer motor
5 | Rear washer switch
6 | Rear wiper and washer switch