#
WHEEL HUB, HUB SPINDLE REMOVAL/INSTALLATION [2WD]

id0312008010a1

  Caution

  • Performing the following procedures without first removing the ABS wheel-speed sensor may possibly cause an open circuit in the harness if it is pulled by mistake. Before performing the following procedures, remove the ABS wheel-speed sensor (body side) and fix it to an appropriate place where the sensor will not be pulled by mistake while the vehicle is being serviced.

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Hub cap
2 | Locknut (See Locknut Removal Note) (See Locknut Installation Note)
3 | Parking brake cable
4 | Brake caliper component
5 | Disc plate (See Disc Plate Removal Note) (See Disc Plate Removal Note)
6 | Wheel hub component
7 | Wheel hub
8 | Hub bolt (See Hub Bolt Removal Note) (See Hub Bolt Installation Note)
9 | ABS sensor rotor (See ABS Sensor Rotor Removal Note) (See ABS Sensor Rotor Installation Note)
10 | Dust cover
11 | Hub spindle

## Locknut Removal Note

1. Knock the crimped portion of the locknut outward using a small cape chisel and a hammer.

2. Lock the hub by applying the brakes.

3. Remove the locknut.

## ABS Sensor Rotor Removal Note

  Note

  • The sensor rotor does not need to be removed unless it is being replaced.

1. Remove the sensor rotor using a chisel.

## ABS Sensor Rotor Installation Note

  Caution

  • Position the SST so that marking B faces the bottom.

1. Set the SST as shown in the figure.

2. Press on the new sensor rotor using the SST and a press.

## Locknut Installation Note

1. Install a new locknut and stake it as shown.