#
DSC HU/CM REMOVAL/INSTALLATION [2WD (ATX), 4WD (MTX)]

id0415008010a9

  Caution

  • When replacing the DSC HU/CM, configuration procedure must be done before removing the DSC HU/CM. If configuration is not completed before removing the DSC HU/CM, DTC B2477 will be detected.
  • The internal parts of the DSC HU/CM could be damaged if dropped. Be careful not to drop the DSC HU/CM. Replace the DSC HU/CM if it is subjected to an impact.

1. Configurate the DSC HU/CM (only when replacing it). (See DSC HU/CM CONFIGURATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Connector (See Connector Removal Note) (See Connector Installation Note
2 | Brake pipe (See Brake Pipe Removal Note) (See Brake Pipe Installation Note)
3 | Nut
4 | DSC HU/CM (See DSC HU/CM Removal/Installation Note)
5 | Stud

## Connector Removal Note

1. Release the lock lever to unlock it.

2. Remove the connector.

## Brake Pipe Removal Note

1. Mark the brake pipe connecting positions before removal for reference during installation.

## DSC HU/CM Removal/Installation Note

1. When removing/installing the DSC HU/CM from/to the vehicle, attach a strip of protective tape on the DSC HU/CM connector to prevent brake fluid from entering.

## Brake Pipe Installation Note

1. When installing the brake pipe, align the marks made before removal with the DSC HU/CM as shown in the figure.

## Connector Installation Note

1. Verify that the lock lever of the harness connector is securely locked.