#
WASTEGATE CONTROL SOLENOID VALVE CONSTRUCTION/OPERATION [L3 Turbo]

id0113b5101300

## Construction

• Mainly composed of the solenoid coil, spring, and plunger.

## Operation

• During energization, the valve opens and performs linear adjustment of the pressure applied to the wastegate actuator releasing it through the air hose.

1 | To air hose
2 | From wastegate actuator
3 | Coil
4 | Spring
5 | Plunger
6 | Air flow