#
NO.5 NO CREEP AT ALL [FS5A-EL]

id050308801000

5 | No creep at all
DESCRIPTION | • Vehicle does not move in D, M ranges and R position when idling on a flat paved road.
POSSIBLE CAUSE | • Either transaxle is stuck in 3GR or 4GR position, or there is clutch circuit slippage due to a stuck 3-4 clutch. 1. Clutch burnt • Line pressure low • Shift solenoid D malfunction • Shift solenoid A malfunction • Shift solenoid B malfunction • Shift solenoid C malfunction • Pressure control solenoid A malfunction • Body GND malfunction • Control valve body malfunction 2. Transaxle fixed in 3GR (Operation of fail-safe function) • Short or open circuit in wiring harness • Poor connection of connector • Malfunction of electronic parts of output and input system 3. There is no engine torque • Torque converter malfunction Note • Before following the troubleshooting steps, make sure that the Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | Does the vehicle creep in any range/position? | Yes | Go to the next step.
No | Inspect or adjust the selector lever. (See SELECTOR LEVER INSPECTION.) (See SELECTOR CABLE ADJUSTMENT.)
2 | Inspect the value at the following TCM PID using the WDS or equivalent. (See TCM INSPECTION [FS5A-EL].) • THOP Is the PID value normal? | Yes | Go to the next step.
No | Repair or replace any malfunctioning parts.
3 | Disconnect the TCM connector. Is the resistance between the ground terminal at the TCM connector and the body ground less than 5.0 ohms? | Yes | Go to the next step.
No | Repair open ground circuit.
4 | Inspect the LPS PID value. Is the LPS PID value normal? (See TCM INSPECTION [FS5A-EL].) | Yes | Overhaul the control valve body and repair or replace any malfunctioning parts. (See ATX workshop manual [FS5A-EL].) If any problem remains, overhaul the transaxle and repair or replace any malfunctioning parts. (See ATX workshop manual [FS5A-EL].)
No | Repair or replace any malfunctioning parts.
5 | • Verify the test results. - If normal, return to the diagnostic index to service any additional symptoms. - If the malfunction remains, inspect the related Service information and perform repair or diagnosis. • If the vehicle is repaired, troubleshooting is completed. • If the vehicle is not repaired or additional diagnostic information is not available, replace the TCM.