#
TRANSFER OIL REPLACEMENT [JA5AX-EL]

id031611800300

1. Remove the drain plug.

2. Drain the oil into a suitable container.

3. Apply a sealant to the thread area of drain plug.

Specified sealant

  TB1215 or equivalent

4. Install the drain plug.

Tightening torque

  9.8-19.6 N·m
  {100-199 kgf·cm, 116-175 in·lbf}

5. Remove the PTO heat shield.

6. Remove the filler plug and add the specified amount and type of oil through the filler plug hole until the level reaches the bottom of the filler plug hole.

Transfer oil [JA5AX-EL]

  Specified oil grade: API Service GL-5
  Specified oil viscosity: SAE 80W-90
  Capacity (approximate quantity): 0.62 L {0.65 US qt, 0.54 lmp qt}

7. Apply a sealant to the thread area of filler plug.

Specified sealant

  TB1215 or equivalent

8. Install the filler plug.

Tightening torque

  9.8-19.6 N·m
  {100-199 kgf·cm, 116-175 in·lbf}

9. Install the PTO heat shield. (See PTO Heat Shield Installation Note.)