#
WOOFER INSPECTION

id092000805100

1. Inspect for continuity between the audio amplifier connector terminals and woofer connector terminals using an ohmmeter.

  • If not as specified, replace the related wiring harnesses.

2. Verify that there is battery positive voltage at the woofer connector terminal A (4SD) or C (5HB, WGN) using a voltmeter.

  • If not as specified, replace the related wiring harness.

3. Inspect continuity between the woofer connector terminal B and body ground using an ohmmeter.

  • If not as specified, replace the related wiring harness.
  • If as specified, replace the woofer.