#
SIDE WINDOW GLASS REMOVAL [WGN]

id0912008038b1

1. Apply protective tape along the edge of the body to protect it from damage.

2. Make a hole through the sealant, avoiding pins, from the inside of the vehicle using an awl.

3. Pass the SST (piano wire) through the hole.

  Warning

  • Using The SST (piano wire) with bare hands can cause injury. Always wear gloves when using the SST (piano wire).

4. Wind each end of the SST (piano wire) around a bar.

  Note

  • Use a long sawing action to spread the work over the whole length of the SST (piano wire) to prevent it from breaking due to localized heating.

5. Fix one end of the SST (piano wire), and while pulling the other end, cut the sealant around the windshield.

6. Remove the side window glass.