#
HEADLIGHT CLEANER NOZZLE REMOVAL/INSTALLATION

id091900808200

1. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

2. Disconnect the headlight cleaner hose. (See HEADLIGHT CLEANER HOSE REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

1 | Screw
2 | Spacer
3 | Headlight cleaner nozzle

4. Install in the reverse order of removal.

5. Adjust the headlight cleaner nozzle. (See HEADLIGHT CLEANER NOZZLE ADJUSTMENT.)