#
THEFT-DETERRENT SIREN OUTLINE

id0914b5870200
• The theft-deterrent siren is located on the rear, left side of the trunk lid (4SD) or liftgate (5HB, WGN).
• Controlled by the following vehicle conditions:

  - Standard alert control
  - Open circuit alert control

## Standard Alert Control

• The siren beeps when receiving an alert initialization signal from the theft-deterrent control module. When a go-to-initial signal is received the siren is stopped.

1 | Theft-deterrent control module
2 | Theft-deterrent siren
3 | Alert initialization signal
4 | Siren beeps

## Open Circuit Alert Control

• A back-up power supply is integrated in the theft-deterrent siren.
• When an open circuit is detected in the related wiring harness, the theft-deterrent siren beeps using the back-up power supply.
• If any one of the following conditions are met, the siren is stopped:

  - Detects that all related wiring harness are propeLRy connected.
  - Receives go-to-initial signal from the theft-deterrent control module.

1 | Theft-deterrent control module
2 | Theft-deterrent siren
3 | Siren beeps
4 | Siren stops
5 | Approx. 30 seconds
6 | Approx. 5 seconds
7 | Maximum 9 cycles