#
CLUTCH PEDAL INSPECTION

id051000801100

## Clutch Pedal Height Inspection

1. Measure the distance from the upper surface of the pedal pad.

Clutch pedal height (with carpet)

  L.H.D. (L8, LF, L3, MZR-CD (RF-Turbo)): 216-222 mm {8.50-8.74 in} (Reference value)
  R.H.D. (L8, LF, L3, MZR-CD (RF-Turbo)): 229-235 mm {9.02-9.25 in} (Reference value)
  L3 Turbo: 210-216 mm {8.27-8.50 in} (Reference value)

2. Adjust the height if necessary. (See Clutch Pedal Height.)

## Clutch Pedal Free Play Inspection

1. Depress the clutch pedal by hand until clutch resistance is felt.

Clutch pedal free play

  1.0-3.0 mm {0.04-0.11 in}

2. Adjust the free play if necessary. (See Clutch Pedal Free Play.)