#
REAR DOOR GLASS REMOVAL/INSTALLATION

id091200415700

1. Fully down the rear door glass.

2. Remove the rear door trim. (See REAR DOOR TRIM REMOVAL/INSTALLATION.)

3. Remove the hole cover.

4. Pull up the rear door weatherstrip and remove the screw.

5. Remove the bolt.

6. Remove the glass run channel from the rear door glass guide.

7. Lift the rear door glass to the position where the rear door glass installation screw is visible.

8. Remove the screw.

9. Insert your hand through the rear door unit hole and lift out the rear door glass.

10. Install in the reverse order of removal.