#
SECONDARY CONTROL VALVE BODY INSTALLATION [FS5A-EL]

id051721807600

## On-Vehicle Installation

1. Install the tubular pin and O-ring to the transaxle case.

2. Install the secondary control valve body component and ground.

Tightening torque

  7.8-10.8 N·m
  {80-110 kgf·cm, 70-95 in·lbf}

Bolt length (measured from below the head)

  B: 40 mm {1.575 in}
  C: 50 mm {1.967 in}

3. Match the harness colors, then connect the solenoid connector.

Spring | Color of connector (harness side)
--- | ---
Pressure control solenoid B | White
Shift solenoid F | Black

4. Apply a light coat of silicon sealant to the contact surfaces of the oil cover and transaxle case.

5. Install the oil cover.

Tightening torque

  7.8-10.8 N·m {80-109 kgf·cm, 70-95 in·lbf}

6. Install the bracket in the figure.

Tightening torque

  18-26 N·m {1.9-2.6 kgf·m, 14-19 ft·lbf}

7. Install the battery and battery tray.

8. Connect the negative battery cable.

9. Add ATF. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [FS5A-EL].)

10. Carry out the mechanical system test. (See MECHANICAL SYSTEM TEST [FS5A-EL].)

11. Carry out the road test. (See ROAD TEST [FS5A-EL].)