#
NO.4 EXCESSIVE CREEP [JA5AX-EL]

id050305800900

4 | Excessive creep
DESCRIPTION | • Vehicle accelerates in D range, and R position without depressing accelerator pedal.
POSSIBLE CAUSE | • Engine idle speed high (transaxle system is not cause of problem) • Go to symptom troubleshooting No.9 "Fast idle/runs on" (See NO.9 FAST IDLE/RUNS ON [L8, LF, L3].) Note • Before following troubleshooting steps, make sure that Automatic Transaxle On-Board Diagnostic and Automatic Transaxle Basic Inspection are conducted.