#
SECONDARY SHAFT COMPONENTS DISASSEMBLY

id051500803400

1. Disassemble in the order indicated in the table.

1 | Bearing (See Bearing and Secondary 4th Gear Disassembly Note.)
2 | Secondary 4th gear (See Bearing and Secondary 4th Gear Disassembly Note.)
3 | Retaining ring
4 | Secondary 3rd gear (See Secondary 3rd Gear and 2nd Gear Disassembly Note.)
5 | Friction damper
6 | 2nd gear (See Secondary 3rd Gear and 2nd Gear Disassembly Note.)
7 | Inner cone
8 | Double cone
9 | 2nd synchronizer ring
10 | Retaining ring
11 | 1st/2nd clutch hub component (See 1st/2nd Clutch Hub Component, 1st Synchronizer Ring, and 1st Gear Disassembly Note.)
12 | 1st synchronizer ring (See 1st/2nd Clutch Hub Component, 1st Synchronizer Ring, and 1st Gear Disassembly Note.)
13 | Double cone
14 | Inner cone
15 | 1st gear (See 1st/2nd Clutch Hub Component, 1st Synchronizer Ring, and 1st Gear Disassembly Note.)
16 | Friction damper
17 | Bearing (See Bearing (Secondary Shaft End) Disassembly Note.)
18 | Secondary shaft gear
19 | Synchronizer key spring
20 | Clutch hub sleeve (reverse gear)
21 | Synchronizer key
22 | 1st/2nd clutch hub

## Bearing and Secondary 4th Gear Disassembly Note

1. Remove the bearing and secondary 4th gear using the SST.

## Secondary 3rd Gear and 2nd Gear Disassembly Note

1. Remove the retaining ring.

2. Shift the gears to 1st gear.

3. Remove the secondary 3rd gear and 2nd gear using the SST.

## 1st/2nd Clutch Hub Component, 1st Synchronizer Ring, and 1st Gear Disassembly Note

1. Remove the retaining ring.

2. Remove the 1st/2nd clutch hub component, 1st synchronizer ring, double cone, inner cone, and 1st gear using a press.

## Bearing (Secondary Shaft End) Disassembly Note

1. Remove the bearing using the SST.