#
SUNROOF MOTOR INSTALLATION

id091500801000

1. Connect the sunroof motor connector.

2. Connect the sunroof switch connector.

3. Connect the negative battery cable.

4. Turn the ignition switch to ON position.

5. Press the CLOSE side of the slide switch until the sunroof motor stops.

6. Disconnect the sunroof switch connector.

7. Install the screws, and then install the sunroof motor.

8. Install the headliner.(See HEADLINER REMOVAL/INSTALLATION [4SD, 5HB].)(See HEADLINER REMOVAL/INSTALLATION [WGN].)

9. Install the net anchor (WGN).

10. Install the assist handle.(See ASSIST HANDLE REMOVAL/INSTALLATION.)

11. Install the sunvisors.(See (SUNVISOR REMOVAL/INSTALLATION.)

12. Install the cargo compartment light (WGN).(See CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION [WGN].)

13. Install the rear map light.(See REAR MAP LIGHT REMOVAL/INSTALLATION.)

14. Install the front map light.(See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

15. Install the D-pillar trims (WGN).(See D-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

16. Install the C-pillar trims.(See C-PILLAR TRIM REMOVAL/INSTALLATION [4SD, 5HB].)(See C-PILLAR TRIM REMOVAL/INSTALLATION [WGN].)

17. Install the B-pillar upper trims.(See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

18. Install the A-pillar trims.(See A-PILLAR TRIM INSTALLATION.)

19. Install the sunroof seaming welt.