#
DISC PAD (FRONT) REPLACEMENT [18 INCH WHEEL]

id0411008007b3

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

.

1 | Bolt
2 | Retaining clip (See Retaining Clip Installation Note.)
3 | Cap
4 | Bolt
5 | Caliper
6 | Disc pad (See Disc Pad Installation Note.)

## Disc Pad Installation Note

1. Push the piston fully inward using the SST.

2. Install the disc pad.