#
EXHAUST SYSTEM OUTLINE [L8, LF, L3]

id0115b1125600
Features
• The exhaust manifold is located behind the engine.
• This layout allows for shorter exhaust pipes and improved exhaust efficiency. Moreover, due to the shorter distance to the catalytic converter, temperature decrease of exhaust emission is prevented and catalyst is more efficient.
• Temperature decrease of exhaust emission is further prevented with double layer exhaust manifold pipes.