#
DTC B1342 [ABS (ABS/TCS)]

id040214809000

DTC | B1342 | ABS (ABS/TCS) HU/CM
DETECTION CONDITION | The on-board diagnostic function detects control module malfunction.
POSSIBLE CAUSE | • Malfunction of ABS (ABS/TCS) HU/CM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear the DTC from the memory. (See Clearing DTCs Procedures.) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above. • Is same DTC present? | Yes | Replace ABS (ABS/TCS) HU/CM, then go to the next step.
No | Inspect intermittent concern using the same procedure as engine control system.
2 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | Troubleshooting completed.