#
STEERING SHAFT INSPECTION

id061400800600

1. Inspect the following.

  (1) Column bearing for damage
  (2) Steering shaft length

  • Replace the steering shaft component as necessary.

Steering shaft length

  211.6 mm {8.3 in}

2. Inspect the tilt and telescope operation

  (1) Verify that the adjusting lever moves smoothly from unlock position to lock position.
  (2) Verify that the steering shaft is fixed firmly when the adjusting lever is locked.

  • Replace the steering shaft component as necessary.