#
DTC B2387

id0902b2844700

DTC B2387 | Ignitor circuit malfunction
DETECTION CONDITION | Warning • Incorrect servicing of the discharge headlight control module could result in electrical shock. Before servicing the discharge headlight control module, always refer to "Discharge headlight service warnings". (See DISCHARGE HEADLIGHT SERVICE WARNINGS) • Ignitor in front combination light is malfunctioning or poorly connected.
POSSIBLE CAUSE | • Ignitor in front combination light is malfunctioning. • Ignitor in front combination light is poorly connected.

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CONNECTOR CONNECTION • Check fit of discharge headlight control module and headlight connectors on both sides (discharge headlight control module (LH) and (RH)). • Are installation condition and fit okay? | Yes | Ignitor in front combination light may be malfunctioning. Replace front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION)
No | After correcting fit, clear DTC and check DTC again. • If DTC is displayed again, replace front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION)