#
DTC B1126 [ADVANCED KEYLESS SYSTEM]

id0902e2350900

DTC B1126 | Steering lock unit internal malfunction.
--- | ---
DETECTION CONDITION | • Detect the steering lock unit maifunction signal.
POSSIBLE CAUSE | • Steering lock unit maifunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT STEERING LOCK UNIT • Turn the ignition switch to the ON position. • Is the DTC displayed? - WDS or equivalent: B1126 | Yes | Replace the steering lock unit and perform the resetting procedure for the steering lock unit. (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.) (See STEERING LOCK UNIT ID CODE REGISTRATION [WITH ADVANCED KEYLESS SYSTEM])
No | DTC troubleshooting completed.