#
ABS (ABS/TCS) CM PART FUNCTION

id041300202900

## Function

• The ABS (ABS/TCS) CM detects the vehicle wheel speeds based on the signals from the four ABS wheel- speed sensors. The CM calculates the rotation condition of each wheel from the relation between the detected vehicle wheel speed and the estimated (based on the detected speed) vehicle speed from there on. It then accordingly controls brake fluid pressure to each wheel to prevent lock-up.

## Function Table

Function name | Contents
--- | ---
ABS control function | • Controls brake fluid pressure when braking to maintain directional stability, ensure steerability and reduce stopping distance.
Electronic brakeforce distribution (EBD) control function | • Constantly controls proper distribution of brake fluid pressure to the front and rear wheels according to vehicle load, road surface and vehicle speed conditions to prevent early lock-up of the rear wheels.
Vehicle speed output function | • Outputs the vehicle speed signal to the Body Control Module (BCM). • Outputs the wheel speed signal and ABS system warning control data via CAN lines.
On-board diagnostic system | • Main components of the ABS control system have a self-diagnosis function. In case a malfunction occurs, warning lights illuminate to alert the driver, and at the same time a DTC is stored in the ABS (ABS/TCS) HU/CM. • When a malfunction is determined as a result of on-board diagnosis, system control is suspended or limited to prevent any dangerous situation while driving.