#
VARIABLE BOOST CONTROL (VBC) CHECK VALVE INSPECTION [MZR-CD (RF Turbo)]

id0113f1777700

1. Remove the VBC check valve. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

2. Blow through port A and verify that the airflows from port B.

  • If not as specified, replace the VBC check valve.

3. Blow through port B and verify that the air does not flow from port A.

  • If not as specified, replace the VBC check valve.