#
SAS CONTROL MODULE REMOVAL/INSTALLATION

id081000801400

  Warning

  • Handling the SAS control module improperly can accidentally deploy the air bag modules and pre-tensioner seat belt, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

  Caution

  • When replacing the SAS unit, configuration procedure must be done before removing the SAS unit. If configuration is not completed before removing the SAS unit, DTC B1017 will be displayed.
  • If configuration is not completed correctly due to some reason, DTCs B1017 and B2477 are displayed.

1. Perform SAS control module configuration when replacing it. (See SAS CONTROL MODULE CONFIGURATIONS.)

2. Turn the ignition switch to the LOCK position.

3. Disconnect the negative battery cable and wait for 1 min or more.

4. Partially peel back the floor covering between the lower panel and console on both the driver and passenger sides.

5. Remove in the order indicated in the table.

  Note

  • L.H.D.
  Remove bolt A from the position where the floor covering between the passenger-side lower panel and console was peeled off, and remove bolt B from the position where the floor covering between the driver-side lower panel and console was peeled off.
  • R.H.D.
  Remove bold A from the position where the floor covering between the driver-side lower panel and console was peeled off, and remove bolt B from the position where the floor covering between the passenger-side lower panel and console was peeled off.

1 | Connector
2 | Bolt A
3 | Bolt B
4 | SAS control module

6. Install in the reverse order of removal.

7. Turn the ignition switch to the ON position.

  • If the SAS control module is replaced, turn the ignition switch to the ON position for 20 s or more after completing the configuration.

8. Verify that the air bag system warning light illuminates for approx. 6 s and goes out.

  • If the air bag system warning light does not operate normally, refer to the on-board diagnostic system (air bag system) and perform inspection of the system.