#
CLUTCH MASTER CYLINDER REMOVAL/INSTALLATION

id051000801400

1. Disconnect the negative battery cable.

2. Remove the battery and battery tray. (European (L.H.D.) specs.)

3. For R.H.D. (L3 Turbo), remove the insulator. (See EXHAUST SYSTEM REMOVAL/INSTALLATION [L3 Turbo].)

4. Remove in the order indicated in the table.

5. Plug the clutch pipe after removing it to avoid leakage.

6. Install in the reverse order of removal.

1 | Clip
2 | Clutch pipe
3 | Nut
4 | Clutch master cylinder
5 | Gasket