#
TRANSAXLE FLUID TEMPERATURE (TFT) SENSOR CONSTRUCTION/OPERATION [JA5AX-EL]

id051705109000
• The TFT sensor is a thermistor type and the resistance changes according to the ATF temperature.
• The characteristic of the resistance is as shown in the figure below.
• The TFT sensor is integrated with the connector.

.

1 | Oil strainer
2 | Magnets
3 | TFT sensor
4 | Increases
5 | Resistance (ohm)
6 | ATF temperature
7 | Characteristic of TFT sensor