VALVE GUIDE REPLACEMENT

id011000501200

Removal

1. Tap the valve guide out from combustion chamber side using the SST.

c3u0110e005

Installation

1. Assemble the SSTs so that dimension L is as specified.

b3e0110e071

  Standard valve guide projection height

  IN: 12.2—12.8 mm {0.481—0.503 in}
  EX: 12.2—12.8 mm {0.481—0.503 in}

2. Tap the valve guide in from the cam side using the SSTs assembled in Step 1.

e6u110zwb061

b3e0110e072