#
SHROUD PANEL REMOVAL/INSTALLATION

id091000406300

1. Remove the bonnet. (See BONNET REMOVAL/INSTALLATION [EXCEPT L3 TURBO].) (See BONNET REMOVAL/INSTALLATION [L3 TURBO].)

2. Remove the front bumper. (See FRONT BUMPER REMOVAL/INSTALLATION.)

3. Remove the front combination light. (See FRONT COMBINATION LIGHT REMOVAL/INSTALLATION.)

4. Remove the front bumper reinforcement. (See FRONT BUMPER REINFORCEMENT REMOVAL/INSTALLATION.)

5. Remove in the order indicated in the table.

1 | Radiator mount cover
2 | Radiator mount rubber
3 | Bolt
4 | Shroud panel

6. Install in the reverse order of removal.