#
FRONT SEAT DISASSEMBLY/ASSEMBLY

id091300800300

  Warning

  • Handling the front seat (side air bag) improperly can accidentally deploy the side air bag, which may seriously injure you. Read AIR BAG SYSTEM SERVICE WARNINGS before handling the front seat. (See SERVICE WARNINGS.) (See SERVICE CAUTIONS.)

1. Disconnect the negative battery cable and wait for more than 1 minute.

2. Remove the side air bag module. (See SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Disassemble in the order indicated in the table.

4. Assemble in the reverse order of disassembly.

## Driver's Seat (Normal Seat)

.

1 | Headrest
2 | Lumber support lever (See Lumber Support Lever Disassembly Note)
3 | Recliner dial (dial type) (See Recliner Dial Disassembly Note) Recliner lever (lever type)
4 | Lift lever outer
5 | Lift lever inner
6 | Front buckle
7 | Side cover (See Side Cover Disassembly Note)
8 | Pole guide
9 | Seat back trim
10 | Seat warmer unit (European (L.H.D.) specs. only)
11 | Seat back pad
12 | Seat back frame
13 | Reverse cover
14 | Seat cushion frame
15 | Seat cushion trim
16 | Seat warmer unit (European (L.H.D.) specs. only)
17 | Seat cushion pad
18 | Slide adjuster

## Driver's Seat (Power Seat)

.

1 | Headrest
2 | Lumber support lever (See Lumber Support Lever Disassembly Note)
3 | Slider and lifter switch knob
4 | Recliner switch knob
5 | Front buckle
6 | Side cover (See Side Cover Disassembly Note)
7 | Position memory switch
8 | Power seat switch
9 | Front cover No. 1
10 | Front cover No. 2
11 | Pole guide
12 | Seat back trim
13 | Seat warmer unit (European (L.H.D.) specs. only)
14 | Seat back pad
15 | Seat back frame
16 | Reverse cover
17 | Seat cushion frame
18 | Seat cushion trim
19 | Seat warmer unit (European (L.H.D.) specs. only)
20 | Seat cushion pad
21 | Slide adjuster

## Passenger's Seat

  Warning

  • Do not disassemble the seat cushion. Doing so will necessitate reassembly which may damage or press the occupancy sensor. This will cause the misoperation of the air bag system, which may seriously injure you.

.

1 | Headrest
2 | Recliner lever
3 | Front buckle
4 | Side cover (See Side Cover Disassembly Note)
5 | Pole guide
6 | Seat back trim
7 | Seat back pad
8 | Seat warmer unit (European (L.H.D.) specs. only)
9 | Seat back frame
10 | Reverse cover
11 | Seat cushion frame
12 | Seat cushion trim
13 | Seat warmer unit (European (L.H.D.) specs. only)
14 | Seat cushion pad
15 | Slide adjuster

## Lumber Support Lever Disassembly Note

1. Remove the pin from the lumber support lever installation part with rag.

## Recliner Dial Disassembly Note

1. Remove the pin from the recliner dial installation part with rag.

## Side Cover Disassembly Note

1. Remove the screws.

2. Disengage the clips.

3. Lift the side cover up in the direction of the arrow, then unhook it from slide adjuster.