#
DTC C1510, C1511, C1512, C1513 [ABS (ABS/TCS)]

id040214874500

DTC | C1510 C1511 C1512 C1513 | RF solenoid valve, motor or RF ABS wheel-speed sensor/ABS sensor rotor. LF solenoid valve, motor or LF ABS wheel-speed sensor/ABS sensor rotor. RR solenoid valve, motor or RR ABS wheel-speed sensor/ABS sensor rotor. LR solenoid valve, motor or LR ABS wheel-speed sensor/ABS sensor rotor.
DETECTION CONDITION | • Wheel lock is detected during ABS operation (pressure reduction inoperative). • Pressure reduction on a single wheel continues for more than 20 seconds.
POSSIBLE CAUSE | • Malfunction of solenoid valve in ABS (ABS/TCS) HU/CM • Malfunction of ABS wheel-speed sensor • Damaged sensor rotor • Stuck pump motor in ABS (ABS/TCS) HU/CM

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY OTHER DTC HAS BEEN RECORDED • Has any ABS wheel-speed sensor, sensor rotor, solenoid valve, pump motor, or motor relay related DTC been output? | Yes | Go to the applicable DTC inspection.
No | Go to the next step.
2 | INSPECT ABS (ABS/TCS) HU/CM OPERATION • Perform ABS (ABS/TCS) HU/CM system inspection. (See ABS (ABS/TCS) HU/CM SYSTEM INSPECTION) • Is it normal? | Yes | Go to the next step.
No | Replace ABS (ABS/TCS) HU/CM, then go to the next step.
3 | VERIFY CURRENT STATUS OF MALFUNCTION • Clear the DTC from the memory. (See Clearing DTCs Procedures) • Start engine and drive vehicle at 10 km/h {6.2 mph} or above at least one minute. • Gradually slow down and stop vehicle. • Is same DTC present? | Yes | Replace ABS (ABS/TCS) HU/CM, then go to the next step.
No | Go to the next step.
4 | VERIFY AFTER REPAIR PROCEDURE • Is there any other DTC present? | Yes | Go to the applicable DTC inspection. (See DTC Table.)
No | Troubleshooting completed.