#
ADVANCED KEYLESS START FUNCTION OPERATION

id0914b5102700
• The advanced start function activates to start the engine by operating the start knob, and not by inserting the key but by carrying the card key in the vehicle.
a. When the start knob is pressed, the keyless control module sends a request signal from the keyless antennas (Interior).
b. The card key receives the request signal, and sends back an ID data.
c. The ID data is received by the keyless receiver, and sent to the keyless control module.
d. When the ID data is verified by the keyless control module and the card key is determined to be inside the vehicle, the start knob of the steering lock unit is released. The keyless indicator light in the instrument cluster illuminates at the same time to indicate that the start knob is operable.

  - If the ID verification is not acceptable (for reasons such as an unprogrammed card key, or card key battery depletion), the start knob is not released and the keyless warning light (red) illuminates to indicate that the start knob is inoperable.
  - For vehicles with the immobilizer system, ID verification is performed when the start knob is turned to the ON position, and if the verification is acceptable, permission is given to start the engine.

e. Turn the start knob to the START position to start the engine.

1 | ID verification NG
2 | Keyless warning light (red) (flash)
3 | ID verification OK
4 | Keyless indicator light (green) (illuminated)
5 | Keyless receiver
6 | Keyless control module
7 | Steering lock unit
8 | Transmitter (card key)
9 | Keyless antenna
10 | Reception range (interior)
11 | 4SD
12 | 5HB, WGN