BATTERY RECHARGING [L8, LF, L3, L3 Turbo]

id0117b1800700

  Warning
  • Keep all flames away from the battery, otherwise evaporated gas from the battery fluid may catch fire, and cause serious injury.
  • Remove the battery filler caps when recharging to prevent battery deformation or damage.

  Caution
  • Do not quick charge for more than 30 min. It will damage the battery.

1. Remove the battery and then place it in a pan of water.

am6zzw00008665

2. Connect a battery charger to the battery and adjust the charging current as follows.

  Battery slow charge current [L8, LF]

  50D20L (40 A·h/5HR, 45 A·h/20HR): 4.0—5.0 A
  50D20L (40 A·h/5HR, 50 A·h/20HR): 4.0—5.0 A
  75D23L (52 A·h/5HR): 5.0—6.0 A

  Battery slow charge current [L3]

  50D20L (40 A·h/5HR, 45 A·h/20HR): 4.0—5.0 A
  50D20L (40 A·h/5HR, 50 A·h/20HR): 4.0—5.0 A
  80D26L (55 A·h/5HR, 65 A·h/20HR): 5.5—6.5 A

  Battery slow charge current [L3 Turbo]

  55D23L (48 A·h/5HR): 4.5—5.5 A
  80D26L (55 A·h/5HR): 5.5—6.5 A

  Battery quick charge current [30 min] [L8, LF]

  50D20L (40 A·h/5HR, 45 A·h/20HR): 25 A
  50D20L (40 A·h/5HR, 50 A·h/20HR): 25 A
  75D23L (52 A·h/5HR): 35 A

  Battery quick charge current [30 min] [L3]

  50D20L (40 A·h/5HR, 45 A·h/20HR): 25 A
  50D20L (40 A·h/5HR, 50 A·h/20HR): 25 A
  80D26L (55 A·h/5HR, 65 A·h/20HR): 35 A

  Battery quick charge current [30 min] [L3 Turbo]

  55D23L (48 A·h/5HR): 30 A
  80D26L (55 A·h/5HR): 35

3. After the battery is recharged, verify that the voltage is within the specification and remains at the same value for 1 h or more after the recharging has been completed.

  • If not within the specification, replace the battery.

  Standard voltage

  12.4 V or more