#
FRONT PILLAR REMOVAL

D6E098074090B01

1. Rough cut area (A), drill the 35 weld locations indicated by (B), then remove the lower part of the front pillar outer.

2. Rough cut area (C), drill the 20 weld locations indicated by (D), and 2 weld locations indicated by (E), then remove the front pillar.

  Note

  • If removing the front pillar reinforcement and the front pillar inner as separate parts, drill 8 locations indicated by (F) and drill 28 locations indicated by (G).