#
DTC B1932

id0902i7844400

DTC B1932 | Auto leveling control module system.
--- | ---
DETECTION CONDITION | Warning • incorrect servicing of the auto leveling control module could result in electrical shock because the unit is integrated with the discharge headlight control module. Before servicing the auto leveling control module, always refer to "Discharge headlight service warnings." (See DISCHARGE HEADLIGHT SERVICE WARNINGS) Auto leveling control module does not work properly.
POSSIBLE CAUSE | • Auto leveling control module malfunction • Poor fit of auto leveling control module

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT AUTO LEVELING CONTROL MODULE CONNECTION • Check fit of auto leveling control module. • Is condition of the fit okay? | Yes | Replace auto leveling control module. (See DISCHARGE HEADLIGHT CONTROL MODULE REMOVAL/INSTALLATION)
No | After correcting fit, clear DTC and check DTC again. • If DTC is displayed again, replace auto leveling control module. (See DISCHARGE HEADLIGHT CONTROL MODULE REMOVAL/INSTALLATION)