#
NO.7 NO SHIFTING [FS5A-EL]

id050308801200

7 | No shifting
DESCRIPTION | • Single shift range only. • Sometimes it shifts correctly.
POSSIBLE CAUSE | • When the gear position is fixed in 3GR due to the fail-safe operation, the malfunction is in the ATX. • Perform malfunction diagnosis according to No.6 "Low maximum speed and poor acceleration". 1. Clutch slippage, burnt • Line pressure low • Shift solenoid D malfunction • Shift solenoid A malfunction • Shift solenoid B malfunction • Shift solenoid C malfunction • Shift solenoid F malfunction • Pressure control solenoid A malfunction • Pressure control solenoid B malfunction • Body GND malfunction • Control valve body malfunction 2. Signal malfunction • Vehicle speed sensor malfunction • Sensor GND malfunction • APP sensor malfunction • TP sensor malfunction • Input/turbine speed sensor malfunction 3. Transaxle fixed in 3GR (Operation of fail-safe function) • Short or open circuit in wiring harness • Poor connection of connector • Disconnected shift solenoid connector • Poor ground of shift solenoid 4. Transaxle fixed in 4GR (Operation of fail-safe function) • Forward clutch slippage • Vehicle speed sensor malfunction • Shift solenoid A malfunction (Stuck on) • Poor connection of connector 5. Transaxle fixed in M range • M range switch malfunction