#
BONNET LATCH SWITCH INSPECTION

id0914z6450000

  Note

  • Bonnet latch switch has a built-in bonnet lock.

1. Open the bonnet.

2. Disconnect the negative battery cable.

3. Remove the radiator grille.

4. Disconnect the bonnet latch switch connector.

5. Inspect for continuity between the bonnet latch switch terminals A and B using an ohmmeter.

  • If there is no continuity, replace the bonnet lock.

6. Lock the bonnet lock using a flathead screwdriver or equivalent as shown.

7. Inspect for continuity between the bonnet latch switch terminals A and B using an ohmmeter.

  • If there is continuity, replace the bonnet lock.

  Caution

  • After the inspection, unlock the bonnet lock. If closing the bonnet with the bonnet lock locked, the bonnet lock and/or bonnet striker may be broken.