#
INTAKE AIR TEMPERATURE (IAT) SENSOR INSPECTION [MZR-CD (RF Turbo)]

id0140f1802200

## Resistance Inspection

1. Disconnect the MAF/IAT sensor connector.

2. Measure the resistance between MAF/IAT sensor terminals D and E using an ohmmeter.

  • If not as specified, replace the MAF/IAT sensor. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])
  • If MAF/IAT sensor is okay, perform the "Circuit Open/Short Inspection".

Specification

Ambient temperature (°C {°F}) | Resistance (kilohm)
--- | ---
20 {68} | 2.21-2.69

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)])

2. Inspect for open/short circuit in the following wiring harnesses.

  • If there is open/short circuit, repair or replace wiring harnesses.

### Open circuit

  • MAF/IAT sensor terminal D and PCM terminal 55
  • MAF/IAT sensor terminal E and PCM terminal 78

### Short circuit

  • MAF/IAT sensor terminal D and power supply
  • MAF/IAT sensor terminal D and body ground
  • MAF/IAT sensor terminal E and power supply