#
BLOWER UNIT DISASSEMBLY/ASSEMBLY

id071100800600

1. Disassemble in the order indicated in the table.

  Caution

  • Apply only the specified grease to the link. Otherwise abnormal noise or improper operation may result.

1 | Air filter cover
2 | Air filter
3 | Blower motor
4 | Air intake actuator
5 | Air intake crank
6 | Air intake door
7 | Polyurethane protector
8 | Blower case (1)
9 | Blower case (2)

2. Assemble in the reverse order of disassembly.