#
UNDERBODY FLAT-PLANE DIMENSIONS

D6E098053010B01

.

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front side frame standard hole | ø16 {0.63}
B | Front crossmember mounting bolt | M14 {0.55}
C | Front side frame standard hole | ø16 {0.63}
D | Front suspension mounting block standard hole | ø59 {2.32}
E | Front crossmember mounting bolt | M14 {0.55}
F | Front frame rear standard hole | ø18 {0.71}
G | Front frame rear standard hole | ø16 {0.63}
H | Front B frame standard hole | ø12 {0.47}
I | Front B frame standard hole | 14 × 20
{0.55 × 0.79}
J | Rear side frame standard hole | ø20 {0.79}
K | Rear crossmember mounting bolt | M14 {0.55}
L | Rear suspension housing bolt | M6 {0.24}
M | Rear crossmember mounting bolt | M14 {0.55}
N | Rear side frame standard hole | 16 × 20
{0.63 × 0.79}