#
DIFFERENTIAL OIL REPLACEMENT [L3]

id0314a3800200

1. Place the vehicle on level ground.

2. Remove the filler plug and washer.

3. Remove the drain plug and drain the differential oil into a container.

4. Install a new washer and the drain plug, and tighten.

Tightening torque

  39-53 N·m {4.0-5.4 kgf·m, 29.0-39.0 ft·lbf}

5. Add the specified differential oil from the filler plug until the level reaches the brim of the plug hole.

Differential oil

  Grade: API service GL-5
  Viscosity: SAE 80W-90
  Capacity (Approximate quantity): 1.00 L {1.06 US qt, 0.88 Imp qt}

6. After filling with differential oil, perform oil level inspection.

7. Install a new washer and the filler plug, and tighten.

Tightening torque

  39.2-53.9 N·m {4.0-5.4 kgf·m, 29.0-39.7 ft·lbf}