#
SHIFT COMPONENT DISASSEMBLY/ASSEMBLY

D6E051517030101

1. Disassemble in the order shown in the figure.

2. Assemble in the reverse order of disassembly.

1 | Guide plate
2 | Knock pin
3 | Spring pin (See Spring Pin Assembly Note.)
4 | Shift lever shaft
5 | Shift lever inner
6 | Inter lock sleeve
7 | Boot
8 | Oil seal (See Shift Lever Shaft Oil Seal Disassembly Note.) (See Shift Lever Shaft Oil Seal Assembly Note.)
9 | Bearing (See Shift Lever Shaft Bearing Disassembly Note.) (See Shift Lever Shaft Bearing Assembly Note.)
10 | Breather plug (See Breather Plug Disassembly Note.) (See Breather Plug Assembly Note.)
11 | Control case
12 | Damper

## Shift Lever Shaft Oil Seal Disassembly Note

1. Remove the oil seal using a flathead screwdriver.

## Shift Lever Shaft Bearing Disassembly Note

1. Remove the bearing using the SST.

## Breather Plug Disassembly Note

1. Remove the breather plug using a pin punch.

## Breather Plug Assembly Note

1. Install the breather plug using the SST.

## Shift Lever Shaft Bearing Assembly Note

1. Install the bearing using the SST.

## Shift Lever Shaft Oil Seal Assembly Note

1. Install the oil seal using the SST.

  • Apply grease to the oil seal lip.

## Spring Pin Assembly Note

1. Tap in a new spring pin shown in the figure.